Common Selections:



Product Line: Ultra,Fin Type: 13/8" Setback, Opening Type: RO, Finish:Ext Sand/Int White,Ener

line: 1

Quantity: 2

Location: Dining

3210U SH U-Factor: .29, SHGC: .22, VT:.51

1/8" SunCoatMAX (Low-E) over 1/8" Clear Flat,Ext Sand/Int White, Colonial Top Only 2W2H Energy Star South-Central

Argon Gas Filled

## f ·

Ii •

ij

'

!

II 1

Size: 32" *x* 54" Net Frame 311/2" X 53 1/2" Dimensions: Sash Height One Half

Model: Single Hung

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer

Hardware: White Hardware, Positive Action Lock Screen: Standard with Fiberglass Mesh

Ratings: STC: 28,OITC: 22, Tested: LC30



Clear Opening W 29 5/16" x H 23 1/8" Sq. Ft. 4.71 Other Ratings: CPD: MIL-A-157-03968-00003

!- !I

Viewed From Exterior

Customer Approva l:

Page 1of 9



**Line:**

2

**Quantity:** 1

1 •

1,1,

!

,I.,

I

**Location:** Stairs

3210U SH U-Factor: .29,SHGC:.22, VT:.51

1/8" SunCoatMAX (Low-E) Tempered over 1/8" Clear Tempered Flat, Ext Sand/Int White, Colonial Top Only 2W2H

Energy Star South-Central Argon Gas Filled

Size: 32" x 54" Net Frame 31 1/2" X 53 1/2" Dimensions: Sash Height One Half Model:Single Hung

Glass: 1/8" SunCoatMAX (Low-E) Tempered over 1/8" Clear Tempered

Other Glass: Gray Foam Spacer

Hardware: White Hardware, Positive Action Lock Screen: Standard with Fiberglass Mesh

Ratings: STC: 28, OITC: 22, Tested: LC30

•

Clear Opening: W 29 5/16" x H 23 1/8" Sq. Ft. 4.71

Other Ratings: CPD: MIL-A-157-03968 -00003

**L'**

Viewed From Exterior

**Line:**

3

**Quantity:** 2

**Location:** Bed 2

3210U SH U-Factor: .29, SHGC:.22, VT: .51

1/8" SunCoatMAX (Low-E) over 1/8" Clear

Fiat,Ext Sand/Int White, Colonial Top Only 2W2H Energy Star South-Central

Argon Gas Filled

·m

i

11

ii

,(,

11

* I

*i*

I

I

I..

.

•

Size: 36" x 60" Net Frame 35 1/2" X 59 1/2"

Dimensions: Sash Height One Half Model:Single Hung

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer

Hardware:White Hardware, Positive Action Lock Screen: Standard with Fiberglass Mesh


Ratings: STC: 28,OITC: 22, Tested: LC30

Clear Opening: W 33 5/16" x H 26 1/8" Sq. Ft. 6.04 Egress: Yes




Other Ratings: CPD: MIL-A-157-03968-00003

Viewed From Exterior

**Customer Approval:**



**Line:** 4



### Quantity: 1

**Location:** UP Landing

3310U PW U-Factor: .28, SHGC: .21,VT: .48

1/8" SunCoatMAX (Low-E) over 1/8" Clear Flat, Ext Sand/Int White, Colonial 2W2H Argon Gas Filled


Size: 24" x 24" Net Frame 23 1/2" X 23 1/2" Model: Picture



Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear


Other Glass: Gray Foam Spacer

! Ratings: STC: 28, OITC: 24, Tested: CW50



I

Other Ratings: CPD:MIL-A-150-03890-00003



Viewed From Exterior

### Customer Approval:

**Line:** 5

### Quantity : 1

**Location:** Up Landing

3210U SH U-Factor: .29,SHGC: .22, VT: .51

1/8" SunCoatMAX (Low-E) over 1/8" Clear

Flat, Ext Sand/Int White, Colonial Top Only 2W2H Energy Star South-Central

Argon Gas Filled

Size: 36" x 60" Net Frame 35 1/2" X 59 1/2" Dimensions: Sash Height One Half



Model:Single Hung

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer

Hardware: White Hardware, Positive Action Lock Screen: Standard with Fiberglass Mesh

•


Ratings: STC: 28,OITC: 22, Tested: LC30



Clear Opening: W 33 5/16" x H 26 1/8" Sq. Ft. 6.04 Egress:Yes

Other Ratings: CPD: MIL-A-157-03968-00003

Viewed From Exterior

### Customer Approval:





line: 6

Quantity: 1

Location:Loft

3210U SH U-Factor: .29, SHGC:.22, VT: .51

1/8" SunCoatMAX (Low-E) over 1/8" Clear Flat,Ext Sand/Int White, ColonialTop Only 2W2H

Argon Gas Filled

, .

Size: 28" x 36" Net Frame 27 1/2" X 35 1/2"

Dimensions: Sash Height One Half Model: Single Hung

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer

Hardware: White Hardware, Positive Action Lock Screen: Standard with Fiberglass Mesh

Ratings: STC: 28, OITC: 22, Tested:LC30

Clear Opening: W 25 5/16" x H 14 1/8" Sq.Ft.2.48 Other Ratings: CPD: MIL-A-157-03968-00003

i,

•

..

Viewed From Exterior

Customer Approva l:

line: 7

Quant ty: 2

Location:master Closet

3210U SH U-Factor: .29,SHGC:.22, VT:.51

1/8" SunCoatMAX (Low-E) over 1/8" Clear Flat,Ext Sand/ Int White, Colonial Top Only 2W2H Argon Gas Filled

Size: 28" x 36" Net Frame 27 1/2" X 35 1/2" Dimensions: Sash Height One Half Model:Single Hung

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer

.I

•

Viewed From Exterior


Hardware: White Hardware,Positive Action Lock



Screen: Standard with Fiberglass Mesh Ratings: STC: 28,OITC: 22, Tested: LC30

Clear Opening: W 25 5/16" x H 14 1/8" Sq. Ft. 2.48

Other Ratings : CPD: MIL-A-157-03968-00003

Customer Approval :





Line: 8

Quantity: 1

Location: Basment Egress

3110U HV U-Factor: .29, SHGC: .22, VT: .51

1/8" SunCoatMAX (Low-E) over 1/8" Clear Energy Star South-Central

Argon Gas Filled

Size: 48" *x* 48" Net Frame 47 1/2" X 47 1/2" Model: Half Vent

Handing: Half Vent XO

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer

Hardware:White Hardware, Positive Action Lock Screen: Standard with Fiberglass Mesh

Ratings: STC: 29, OITC: 23, Tested: LC30

Clear Opening: W 20 1/8" x H 45 5/16" Sq. Ft. 6.33 Egress:Yes

Other Ratings: CPD: MIL-A-158-05022-00003

Viewed From Exterior

Customer Approval :

Line: 9

Quantity: 2

Location: Bed 2

3210U SH U-Factor: .29, SHGC: .22, VT: .51

1/8" SunCoatMAX (Low-E) over 1/8" Clear Energy Star South-Central

Argon Gas Filled

;iii

. ;

•

Viewed From Exterior

Size: 36" *x* 60" Net Frame 35 1/2" X 59 1/2"

Dimensions: Sash Height One Half Model: Single Hung

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer

Hardware: White Hardware, Positive Action Lock Screen: Standard with Fiberglass Mesh Ratings:STC: 28,OITC: 22, Tested: LC30




Clear Opening: W 33 5/16" x H 26 1/8" Sq. Ft. 6.04

Egress: Yes

Other Ratings: CPD: MIL-A-157-03968-00003

Customer Approval :





Line:

10

Quantity: 1

Location: Laundry

3210U SH U-Factor: .29, SHGC: .22, VT: .51

1/8" SunCoatMAX (Low-E) over 1/8" Clear Argon Gas Filled

•

Viewed From Exterior

Size: 24" x 36" Net Frame 23 1/2" X 35 1/2"

Dimensions:Sash Height One Half Model: Single Hung

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer

Hardware: White Hardware,Positive Action Lock Screen:Standard with Fiberglass Mesh

Ratings: STC: 28,OITC: 22, Tested: LC30

Clear Opening: W 215/16" x H 14 1/8" Sq. Ft. 2.09 Other Ratings: CPD: MIL-A-157-03968-00003

Customer Approval :

Line: 11

Quantity : 4

Location: Great Room

3310U PW U-Factor: .28,SHGC: .23, VT: .53

1/8" SunCoatMAX (Low-E) over 1/8" Clear Energy Star South-Central

Argon Gas Filled

Size: 36" x 76" Net Frame 35 1/2" X 75 1/2" Model:Picture

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer


Ratings: STC: 28, OITC:24, No Ratings

Other Ratings: CPD: MIL-A-150-03889-00003



Viewed From Exterior

Customer Approval:

Page 6 of 9



Line: 12



Quantity: 1

Location: Master Tub

3310U PW U-Factor: .28, SHGC: .23, VT: .53

1/8" SunCoatMAX (Low-E) Tempered over 1/8" Clear Tempered Argon Gas Filled

Size: 36" *x* 18" Net Frame 35 1/2" X 17 1/2" Model: Picture

Glass: 1/8" SunCoatMAX (Low-E) Tempered over 1/8" Clear Tempered

Other Glass: Gray Foam Spacer

Ratings: STC: 28, OITC: 24,Tested:CW50 Other Ratings: CPD: MIL-A-150-03889-00003

Viewed From Exterior

Line: 13

Quantity: 1

Location: Master Bed

3210U SH U-Factor: .29, SHGC: .22, VT: .51

1/8" SunCoatMAX (Low-E) over 1/8" Clear Energy Star South-Central

Argon Gas Filled

·,11 '

·1

Size: 48" x 56" Net Frame 47 1/2" X 55 1/2" Dimensions: Sash Height One Half

Model: Single Hung

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear

·i11

-l Other Glass: Gray Foam Spacer

. (

I! 1

I

•

## 1 1

J • 1r

Hardware: White Hardware, Positive Action Lock

Screen: Standard with Fiberglass Mesh Ratings:STC: 28, OITC: 22, Tested: LC30


Clear Opening: W 45 5/16" *x* H 24 1/8" Sq. Ft. 7.59

Egress: Yes

Other Ratings: CPD: MIL-A-157-03968-00003

Viewed From Exterior

Customer Approval :



**Line:** 14

#### Quantity: 2

**Location:** Bed 3 & 4

3210U SH U-Factor: .29, SHGC: .22, VT: .51

1/8" SunCoatMAX (Low-E) over 1/8" Clear Energy Star South-Central

Argon Gas Filled

# •



Viewed From Exterior

Size: 36" x 60" Net Frame 35 1/2" X 59 1/2" Dimensions: Sash Height One Half

Model: Single Hung

Glass: 1/8" SunCoatMAX (Low-E) over 1/8" Clear Other Glass: Gray Foam Spacer

Hardware: White Hardware, Positive Action Lock Screen: Standard with Fiberglass Mesh

Ratings: STC: 28,OITC: 22, Tested: LC30

Clear Opening: W 33 5/16" x H 26 1/8" Sq. Ft. 6.04 Egress: Yes

Other Ratings: CPD: MIL-A-157-03968-00003

#### Customer Approval:

**Line:** 15

#### Quantity: 1

**Location:**




3642U IS2P2 U-Factor: .26,SHGC:.16, VT: .37

1/8" SunCoatMAX (Low-E) Tempered over 1/8" Clear Tempered Energy Star South-Central


Handle Finish: Ext Satin Nickel/Int Satin Nickel Hinge Finish: Satin Nickel

Sill Cover

Foam fill Frame Argon Gas Filled



* **0** T



,, ,

**1**...

Viewed From Exterior

Size: 72" x 82" Net Frame 711/2" X 811/2"

J

Model: lnswing Two Panel

11 Handing: AP

I

Glass: 1/8" SunCoatMAX (Low-E) Tempered over 1/8"



Clear Tempered

Other Glass: Gray Foam Spacer

Wall Condition: 4 9/16" Wall Condition

Hardware: Madrona Handle, Ext Satin Nickel,Int Satin Nickel,Satin Nickel Hinge Finish

Other Options: Standard Sill,Construction Sill Cover Screen: Standard with Fiberglass Mesh

Ratings: STC:29, OITC: 24, Tested: LC50

Clear Opening: W 63 3/4" H 77 1/2" Sq. Ft. 34.31 Egress: Yes

Other Ratings: CPD: MIL-A-242 -09972-00007

#### Customer Approval: